Properly make step sequencer, probably do 8 or 16 bars worth. Actually have 2 sequencers so the user can modulate different parameters separately with either one. Have it so each step sequencer can send its triggers to 4 locations total (not 4 total options for where to send it, but the triggers can effect 4 different parameters at once). Additionally have it so the sequencers can be linked (i.e. sequence on 1 = sequence on 2) so the user can instead effectively be able to send one sequencer to 8 locations.